

**THE ZOO**

**Production Manager: Eddie Gresack:** [**eddie.gresack@qmusic.com.au**](mailto:eddie.gresack@qmusic.com.au)

**Artist Liaison:**

**PRODUCTION**

**FOH:**

**FOH CONTROL**  Avid VENUE SC48

– 3 x AI16 input cards (48ch inputs)

– 2 x AO16 outputs cards (32ch outputs)

1 x Klark Teknik DN 360 EQ

2 x dbx 160A compressor/limiter (in-line over FOH)

2 x BSS FDS366 system processor

1 x Furman PL-plus power conditioner

31 channel multicore from stage to FOH, with split to monitor console

FOH PA

Stereo Active 4-way system

4 x Turbosound TA500 (active 3-way)

6 x JBL system 1200 sub cabinets

2 x AM 2200 tri-amp

3 x AM 3002 power amp

31 channel multicore from stage to FOH, with split to monitor console

**MONITORS:**

**MONITOR CONTROL:** Soundcraft Si1 (32 XLR Inputs, 16 16XLR Outputs

2 x BSS FDS334 System Processors

1 x Active Monitor (listen wedge)

**MONITOR SYSTEM:** 3 pairs of active wedges and an active drumfill (4 sends)

6 x active wedges across front of stage (15” + 2” horn)

1 x active drumfill (2 x 15” + 2” horn)

2 x AM 1k2 Power Amp

1 x AM 1600 Power Amp

1 x AM 3002 Power Amp

1 x AM 2200 Power Amp (Listen Wedge)

**MIC KIT:** 1 x beta 52

4 x beta 57

2 x SM57

6 x SM58

3 x Sennheiser 604

3 x Rode NT5

8 x BSS active DI

**STANDS**

2 x Z-Bars

3 x Drum Claws – Konig & Meyer

18 x Mic Stands – 8 x short, 8 x tall, 2 x straight

**LIGHTING:** 1 x LSC 24/48 lighting console

1 x 12 ch Jands Dimmer rack

1 x Analogue 12 ch Dimmer rack (digital-analogue converter supplied)

14 x par 64 (8 on front bar, 6 on sides)

8 x par 56 (rear lighting trees)

4 x LED par64 (rear upright truss)

3 x 800w Fresnel

**BACKLINE:**

1 x Fender Deville (Hot Rod III) 4 x 10″ combo

1 x Ashdown ABM-600 bass head

1 x Ashdown 6 x 10″ speaker cabinet

Truth Custom Drumkit including:–

1 x 24″ Kick

1 x 13″ Rack Tom w/ stand mount

1 x 18″ Floor Tom

1 x 14″ Snare

3 x Boom type cymbal stands

Hi-hat stand w/ clutch

Kick pedal

**DJ EQUIPMENT:**

1x Pioneer DJM-900NXS Nexus 4-channel DJ Mixer

2x Pioneer CDJ900NXS DJ Multiplayer

**STAGE SIZE:**

● 6m wide x 5m deep incl. 600mm proscenium

● 1m high stage, 3m stage floor-to-ceiling

● 6m wide x 500mm long border drape above proscenium

● 500mm wide x 3m long foldable leg drapes at proscenium edges