

**MANE (Woolly Mammoth)**

**Stage Manager**:

**Venue Liaison**:

**Production Manager**: Ed Gresack / eddie.gresak@qmusic.com.au

**Artist Liaison**:

**PRODUCTION**

**FOH CONSOLE** Midas M32

34/6 Analogue Core

Mons from FOH

**FOH SYSTEM** 10 x TLA 308 Line array elements

5 x Box per side run 3 way

4 x RCF AT dual 18” Sub Speaker (L18P300 Loaded)

1 x Powersoft X8 Amplifier

Powersoft Armonia Pro Audio Suite processing (Locked)

41,600 watts FOH

**MONITOR SYSTEM** 6 x QUEST 12MP

2 x Turbosound TXD 252 (Drum Fill/Side Fill)

1 x Active RCF box

1 x Powersoft M50Q HDSP+ETH Amp

1 x Camco D4 power Amp

8,800 Watts MONS

**LIGHTING – To view patch list-**

**https://www.dropbox.com/sh/zaf4sjzkfjru0pi/AAAajpjSGG8vsN1Bg8\_8hMHGa?dl=0**

ChamSys MagicQ

Chamys Magic Q Mini wing control surface

24-inch touch screen computer

Jands 4pak running 4x Par 56 open (Wash)

3 x 3 metre truss rigged left to right far upstage, downstage edge and over the dance floor.

8 x RGB LED Can - 7 channel mode

1 x 1200 watt strobe

2 x 3000 watt Strobes (Wings of stage, floor)

2 x 575 Moving head spot - 16 channel mode

5 x iMove 250 moving head spot - 16 channel mode

2 x Sunstrips - 75watt blubs

1x Chauvet Hurricane 2D haze machine

**PROJECTION**

2K lumen EPSON EB-W6 Mounted on extension to down-stage truss (HDMI AT FOH + VGA AT STAGE).

**STAGING**

Stage size: 6.3m wide x 3.7m deep x 3.4m high

PA Wings: PA Flown Downstage edge with Subs in a cluster in the centre under the stage

Punter Barrier: None

**MICS/LEADS/STANDS**

•5x Shure SM58

•3x Sennheiser 835

•2x Sennhesier 845

•1x Sennheiser 901

•1x Sennheiser 602

•1x Shure Beta 52

•7x Sennheiser 604

•5x Shure SM57

•2x Sennheiser 609

•2x Samson CO2 pencil condensors

•8x Klark Teknik DN100 active DI

•1x Klark Teknik DN200 active DI (stereo)

•6 x short boom mic stands

•10 x tall boom mic stands

•50 x 3-10m XLR cables

**POWER**

1 x 32 Amp 3 phase power for Audio (USED)

1 x 32 Amp 3 Phase power for Lighting/Other (UN-USED)

1 x 3 phase electricians Distro box, 6 points available (UN-USED)

10 amp 240v GPO’s located at various points around stage (16 amp breakers)

**DJ SYSTEM**

2 x Pioneer CDJ 2000nexus

1 x Pioneer DJM900 Nexus

DJ Table- 2.4m x 1.2m 900mm high (Global Stage)

**-----ALL DJs NEED TO BRING THEIR OWN NEEDLES & SLIPMATS-----**

**BACKLINE**

**Pearl Reference Pure Drum Kit (Scarlet Sparkle Burst)**

**22, 10, 12, 16, all hdwr & rug**

**Ampeg SVT Classic, Ampeg 610HLF**

**Fender Deville 212**

**Fender ’65 Twin**

**2x single tier keyboard stand**

**1x double tier keyboard stand**

**3x gtr stands**